Preconfigure new WAN router. New configuration will be applied to the new router on Tuesday

Rack and pre cable WAN router

Trace cabling for existing systems

Mute SW alerts

Capture before

Reboot lodge core

Confirm the status of the core after the reboot

Verify services after reboot

Apply Camp vrf configuration

Verify services after

Correct any issues

Move connections to the new WAN router

Verify routing and services after

Recable the environment to bypass the no longer in use equipment

Verify services after

Correct any issues

Remove systems no longer in use; exinda, DMZ switches, WLCs, Riverbed, etc